|  |  |  |
| --- | --- | --- |
| **Vessel :****BITU ATLANTIC** | **Date(dd/mm/yy) :****14.11.2020** | **Department:****ENGINE** |

|  |  |  |  |
| --- | --- | --- | --- |
| **Name Of Equipment:** | A/E LO. PURIFIER | **Maker:** | MITSUBISHI SELFJECTOR |
| **Type Of Equipment:** |  | **Serial No:** | SJ30G |
| **Report No:** |  | **Running Hrs:** |  |

|  |
| --- |
| **Reason For Work:** |
| PLANNED MAINTENANCE |
|  |
|  |
|  |
|  |

|  |
| --- |
| **Details Of Work Done:** |
| Checked and cleaned frame trap for gear contamination, sludge deposits, y-strainer.Solenoid v/v checked for scaling and diaphragm are in good condition and constant flow v/v checked. Brake linings checked. Operating water drain outlet made clear and alarms tested for discharge detector. Sump oil renewed and foundation bolts retightened. |
|  |
|  |
|  |
|  |
|  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Spare Parts Used:** |  |  |  |
| **P/N** | **Description** | **Qty** | **Qty Rob** |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Planned Maintenance Items Done:** | | | |
| **Code** | **O/H Date** | **Hrs At O/H** | **Remarks** |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Completed:** | | | |
| **Date:** | 14.11.2020 | **Name:** | GURPREET SINGH |
| **Rank:** | 4TH Eng | **Signature:** |  |